configuration / chassis0 / slots / [SLOT-ID] / [hps100] / module / ptpv2 / instances / instance[ID] / global
CLI REST-API

## ptp-unicast-ip-address-2

IP address of Grandmaster 2
This is a read-write object and valid values are IPv4-addresses.
Datatype-Help:
the IP address should looks like this: A.B.C.D
every letter is one number that goes from 0 - 255.
example: 192.168.0.45

#### Applies to modules

HPS100
See also:
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global/ptp-mode
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global/delay-mechanism
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global/domain-number
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global/timescale
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global/priority-1
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global/priority-2
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global/sync-interval
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global/announce-interval
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global/delay-request-interval
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global/ptp-unicast-interval-duration
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global/ptp-hybrid-mode
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global/profile-preset
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global/network-protocol
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global/announce-receipt-timeout
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global/profile-specific-extension
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global/ptp-unicast-ip-address-1
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global/ptp-enable-alt-priority1-2
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global/alt-priority2

#### REST-API Support:

This object is supported by the REST API:
Method: GET
URL: /api/configuration/chassis0/slots/.*/module/ptpv2/instances/instance.*/global
Example using curl:

    curl /api/configuration/chassis0/slots/.*/module/ptpv2/instances/instance.*/global

Method: PATCH
URL: /api/configuration/chassis0/slots/.*/module/ptpv2/instances/instance.*/global
Body:

    {
      "ptp-unicast-ip-address-2": "0.0.0.0"
    }

Example using curl:

    curl -X PATCH /api/configuration/chassis0/slots/.*/module/ptpv2/instances/instance.*/global -d
    {
      "ptp-unicast-ip-address-2": "0.0.0.0"
    }