configuration / chassis0 / slots / [SLOT-ID] / [gps190] / module / gps / serial-ports / com[ID]
CLI REST-API

## baudrate

Baudrate
This is a read-write object and valid values are:

- none [-1]
- 300 [0]
- 600 [1]
- 1200 [2]
- 2400 [3]
- 4800 [4]
- 9600 [5]
- 19200 [6]
- 38400 [7]
- 57600 [8]
- 115200 [9]
- 230400 [10]
- 460800 [11]
- 921600 [12]

#### Applies to modules

GPS167
GPS167SV
GPS170
GPS180
GNS181_UC
GPS190
GNS181
GNS190
See also:
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/gps/serial-ports/com[ID]
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/gps/serial-ports/com[ID]/framing
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/gps/serial-ports/com[ID]/mode
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/gps/serial-ports/com[ID]/string-type

#### REST-API Support:

This object is supported by the REST API:
Method: GET
URL: /api/configuration/chassis0/slots/.*/module/gps/serial-ports/com.*
Example using curl:

    curl /api/configuration/chassis0/slots/.*/module/gps/serial-ports/com.*

Method: PATCH
URL: /api/configuration/chassis0/slots/.*/module/gps/serial-ports/com.*
Body:

    {
      "baudrate": "none"
    }

Example using curl:

    curl -X PATCH /api/configuration/chassis0/slots/.*/module/gps/serial-ports/com.* -d
    {
      "baudrate": "none"
    }