status / chassis0 / slots / [SLOT-ID] / [gnm181] / module / info / sensors
CLI REST-API

## current-board-supply-1

current board supply 1
This is a read-only object and valid values are floating point numbers.

#### Applies to modules

GPS167
GPS167SV
PZF511
GPS170
TCR511
AM511
MSF511
GRC170
WWVB511
MGR170
JJY511
PZF600
TCR600
GPS180
GLN170
MGR180
MSF600
WWVB600
JJY600
ESI180
CPE180
LNO180
GRC180
LIU
MRI
BPE
RSC180
LNE_GB
SCG
FDM180
SPT
PZF180
REL1000
HPS100
VSG180
MSF180
WWVB180
CPC180
TCR180
LUE180
SCU_01
LNE180SFP
GTS180
GRC181
GNS181_UC
PSX210
CPC200
FDM180M
LSG180
GPS190
GNS181
PIO180
SSP100
VSI180
GNM181
RSC2000
REL1000_RC
VSG181
BPE2XXX
BPE2352
BPE8XXX
BPE6042
GNS190
CPU
CES
See also:
/status/chassis0/slots/[SLOT-ID]/[am511]/module/info/sensors
/status/chassis0/slots/[SLOT-ID]/[am511]/module/info/sensors/temperature-1
/status/chassis0/slots/[SLOT-ID]/[am511]/module/info/sensors/voltage-1
/status/chassis0/slots/[SLOT-ID]/[am511]/module/info/sensors/control-voltage-1
/status/chassis0/slots/[SLOT-ID]/[am511]/module/info/sensors/voltage-input-1
/status/chassis0/slots/[SLOT-ID]/[am511]/module/info/sensors/voltage-output-1
/status/chassis0/slots/[SLOT-ID]/[am511]/module/info/sensors/voltage-supply-1
/status/chassis0/slots/[SLOT-ID]/[am511]/module/info/sensors/current-1
/status/chassis0/slots/[SLOT-ID]/[am511]/module/info/sensors/current-osc-supply-1
/status/chassis0/slots/[SLOT-ID]/[am511]/module/info/sensors/simple-input-switch-sensor-1
/status/chassis0/slots/[SLOT-ID]/[am511]/module/info/sensors/simple-output-switch-sensor-1
/status/chassis0/slots/[SLOT-ID]/[am511]/module/info/sensors/uptime-1
/status/chassis0/slots/[SLOT-ID]/[am511]/module/info/sensors/rf-power-1

#### REST-API Support:

This object is supported by the REST API:
Method: GET
URL: /api/status/chassis0/slots/.*/module/info/sensors
Example using curl:

    curl /api/status/chassis0/slots/.*/module/info/sensors