status / chassis0 / slots / [SLOT-ID] / [am511] / module / dcf77
CLI REST-API

## receiver

The submenu receiver (receiver) contains the following:
Menus: none
Objects:
freerunning (long wave or time code receiver running on xtal, satellite receiver has not verified its position)
daylight-savings-time (daylight saving currently enabled)
synchronized-after-reset (long wave or time code receiver has sync'ed at least once after pwr up, sat receiver is synchronized)
daylight-savings-time-announced (a change in daylight saving status is announced)
utc-timescale (returned time is always UTC instead of some local time)
leapsecond-announced (leapsecond announced)
manual-time (the current time has been set by an API call)
invalid-time (invalid time because battery had been disconnected, or absolute time can not be decoded safely)
Commands: none

#### Applies to modules

PZF511
AM511
PZF600
PZF180
See also:
/status/chassis0/slots/[SLOT-ID]/[am511]/module/dcf77/receiver/freerunning
/status/chassis0/slots/[SLOT-ID]/[am511]/module/dcf77/receiver/daylight-savings-time
/status/chassis0/slots/[SLOT-ID]/[am511]/module/dcf77/receiver/synchronized-after-reset
/status/chassis0/slots/[SLOT-ID]/[am511]/module/dcf77/receiver/daylight-savings-time-announced
/status/chassis0/slots/[SLOT-ID]/[am511]/module/dcf77/receiver/utc-timescale
/status/chassis0/slots/[SLOT-ID]/[am511]/module/dcf77/receiver/leapsecond-announced
/status/chassis0/slots/[SLOT-ID]/[am511]/module/dcf77/receiver/manual-time
/status/chassis0/slots/[SLOT-ID]/[am511]/module/dcf77/receiver/invalid-time

#### REST-API Support:

This menu is supported by the REST API:
Method: GET
URL: /api/status/chassis0/slots/.*/module/dcf77/receiver
Example using curl:

    curl /api/status/chassis0/slots/.*/module/dcf77/receiver