configuration / chassis0 / slots / [SLOT-ID] / [gns181_uc] / module / ppo / ppo[ID]
CLI REST-API

## mode

mode
This is a read-write object and valid values are:

- idle [0] (Idle)
- timer [1] (Timer)
- single-shot [2] (Single Shot)
- cyclic-pulse [3] (Cyclic Pulse)
- pulse-per-second [4] (Pulse Per Second)
- pulse-per-min [5] (Pulse Per Min)
- pulse-per-hour [6] (Pulse Per Hour)
- dcf77-marks [7] (DCF77 Marks)
- position-ok [8] (Position OK)
- time-sync [9] (Time Sync)
- all-sync [10] (All Sync)
- dcls-time-code [11] (DCLS Time Code)
- serial-time-string [12] (Serial Time String)
- 10-mhz-frequency [13] (10 MHz Frequency)
- dcf77-like-m59 [14] (DCF77-like M59)
- synthesizer-frequency [15] (Synthesizer Frequency)
- time-slots-per-minute [16] (Time Slots per Minute)
- gpio-signal [17] (GPIO Signal)
- ptti-1-pps [18] (PTTI 1 PPS)
- havequick [19] (HaveQuick)
- 1-mhz-frequency [20] (1 MHz Frequency)
- 5-mhz-frequency [21] (5 MHz Frequency)
- bcd-timecode [22] (BCD TIMECODE)
- 48-khz-clk-out [23] (48 kHz clock output)
- 44_1-khz-clk-out [24] (44.1 kHz clock output)

#### Applies to modules

GPS167
GPS167SV
GPS170
GPS180
GNS181_UC
GPS190
GNS181
GNS190
See also:
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/ppo/ppo[ID]
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/ppo/ppo[ID]/length-s
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/ppo/ppo[ID]/length-ms
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/ppo/ppo[ID]/output-level
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/ppo/ppo[ID]/output-holdover
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/ppo/ppo[ID]/timeout

#### REST-API Support:

This object is supported by the REST API:
Method: GET
URL: /api/configuration/chassis0/slots/.*/module/ppo/ppo.*
Example using curl:

    curl /api/configuration/chassis0/slots/.*/module/ppo/ppo.*

Method: PATCH
URL: /api/configuration/chassis0/slots/.*/module/ppo/ppo.*
Body:

    {
      "mode": "idle"
    }

Example using curl:

    curl -X PATCH /api/configuration/chassis0/slots/.*/module/ppo/ppo.* -d
    {
      "mode": "idle"
    }