configuration / chassis0 / slots / [SLOT-ID] / [gns181] / module / mrs
CLI REST-API

## ref

The submenu ref (REF) contains the following:
Menus: none
Objects:
max-time-deviation-follow (Max Time Deviation to follow)
max-time-deviation-warmed-up (Max Time Deviation keep warmed_up)
max-step-size-first-sync (Max Step Size after first sync)
max-correction-transition (Max Correction in Transition Mode)
max-correction-warmed-up (Max Correction in warmed_up Mode)
Commands: none

#### Applies to modules

GPS167
GPS167SV
GPS170
GPS180
PZF180
GNS181_UC
GPS190
GNS181
GNS190
See also:
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/mrs/ref/max-time-deviation-follow
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/mrs/ref/max-time-deviation-warmed-up
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/mrs/ref/max-step-size-first-sync
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/mrs/ref/max-correction-transition
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/mrs/ref/max-correction-warmed-up

#### REST-API Support:

This menu is supported by the REST API:
Method: GET
URL: /api/configuration/chassis0/slots/.*/module/mrs/ref
Example using curl:

    curl /api/configuration/chassis0/slots/.*/module/mrs/ref

Method: PATCH
URL: /api/configuration/chassis0/slots/.*/module/mrs/ref
Body:

    {
      \"objects\": \"new-values\"
    }

Example using curl:

    curl -X PATCH /api/configuration/chassis0/slots/.*/module/mrs/ref
    -d "{
      \"objects\": \"new-values\"
    }"