configuration / chassis0 / slots / [SLOT-ID] / [gps180] / module
CLI REST-API

## havequick

The submenu havequick (HaveQuick) contains the following:
Menus: none
Objects:
tx-format (TX format)
tx-inverted (TX inverted)
tx-gen-local-time (TX gen local time)
rx-format (RX format)
rx-min-tfom (RX min tfom (-1 = disabled))
rx-inverted (RX inverted)
rx-external-pps (RX external PPS)
rx-offset (RX offset in seconds)
Commands: none

#### Applies to modules

GPS167
GPS167SV
GPS170
GPS180
GNS181_UC
GPS190
GNS181
GNS190
See also:
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/havequick/tx-format
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/havequick/tx-inverted
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/havequick/tx-gen-local-time
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/havequick/rx-format
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/havequick/rx-min-tfom
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/havequick/rx-inverted
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/havequick/rx-external-pps
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/havequick/rx-offset

#### REST-API Support:

This menu is supported by the REST API:
Method: GET
URL: /api/configuration/chassis0/slots/.*/module/havequick
Example using curl:

    curl /api/configuration/chassis0/slots/.*/module/havequick

Method: PATCH
URL: /api/configuration/chassis0/slots/.*/module/havequick
Body:

    {
      \"objects\": \"new-values\"
    }

Example using curl:

    curl -X PATCH /api/configuration/chassis0/slots/.*/module/havequick
    -d "{
      \"objects\": \"new-values\"
    }"