configuration / chassis0 / slots / [SLOT-ID] / [hps100] / module / sync-e
CLI REST-API

## fixed-input-ssm

fixed-input-ssm
This is a read-write object and valid values are:

- ql-prc [2]
- ql-ssu-a [4]
- ql-ssu-b [8]
- ql-sec [11]
- ql-dnu [15]

#### Applies to modules

HPS100
See also:
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/sync-e
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/sync-e/enable-sync-e
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/sync-e/quality-level-selection
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/sync-e/sdh-network-option
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/sync-e/fixed-output-ssm
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/sync-e/gbit-link-copper-mode

#### REST-API Support:

This object is supported by the REST API:
Method: GET
URL: /api/configuration/chassis0/slots/.*/module/sync-e
Example using curl:

    curl /api/configuration/chassis0/slots/.*/module/sync-e

Method: PATCH
URL: /api/configuration/chassis0/slots/.*/module/sync-e
Body:

    {
      "fixed-input-ssm": "ql-prc"
    }

Example using curl:

    curl -X PATCH /api/configuration/chassis0/slots/.*/module/sync-e -d
    {
      "fixed-input-ssm": "ql-prc"
    }