configuration / chassis0 / slots / [SLOT-ID] / [hps100] / module / ptpv2 / instances / instance[ID] / global
CLI REST-API

## ieee-802-1as

The submenu ieee-802-1as (IEEE-802.1AS) contains the following:
Menus: none
Objects:
use-profile-extensions (use-profile-extensions)
Commands: none

#### Applies to modules

HPS100
See also:
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global/ieee-802-1as/use-profile-extensions

#### REST-API Support:

This menu is supported by the REST API:
Method: GET
URL: /api/configuration/chassis0/slots/.*/module/ptpv2/instances/instance.*/global/ieee-802-1as
Example using curl:

    curl /api/configuration/chassis0/slots/.*/module/ptpv2/instances/instance.*/global/ieee-802-1as

Method: PATCH
URL: /api/configuration/chassis0/slots/.*/module/ptpv2/instances/instance.*/global/ieee-802-1as
Body:

    {
      \"objects\": \"new-values\"
    }

Example using curl:

    curl -X PATCH /api/configuration/chassis0/slots/.*/module/ptpv2/instances/instance.*/global/ieee-802-1as
    -d "{
      \"objects\": \"new-values\"
    }"