configuration / chassis0 / slots / [SLOT-ID] / [lue180] / module / ports / port[ID]
CLI REST-API

## e1

The submenu e1 (e1) contains the following:
Menus: none
Objects:
min-quality-level (minimum E1 SSM for acceptance)
sa-bits (sa bits group carrying SSM)
Commands: none

#### Applies to modules

GPS167
GPS167SV
PZF511
GPS170
TCR511
AM511
MSF511
GRC170
WWVB511
MGR170
PZF600
TCR600
GPS180
GLN170
MGR180
MSF600
WWVB600
ESI180
CPE180
LNO180
GRC180
LIU
MRI
BPE
RSC180
LNE_GB
SCG
FDM180
SPT
PZF180
REL1000
HPS100
VSG180
MSF180
WWVB180
CPC180
TCR180
LUE180
SCU_01
LNE180SFP
GTS180
GRC181
GNS181_UC
PSX210
CPC200
FDM180M
LSG180
GPS190
GNS181
PIO180
SSP100
VSI180
GNM181
RSC2000
REL1000_RC
VSG181
BPE2XXX
BPE2352
BPE8XXX
BPE6042
GNS190
CES
See also:
/configuration/chassis0/slots/[SLOT-ID]/[am511]/module/ports/port[ID]/e1/min-quality-level
/configuration/chassis0/slots/[SLOT-ID]/[am511]/module/ports/port[ID]/e1/sa-bits

#### REST-API Support:

This menu is supported by the REST API:
Method: GET
URL: /api/configuration/chassis0/slots/.*/module/ports/port.*/e1
Example using curl:

    curl /api/configuration/chassis0/slots/.*/module/ports/port.*/e1

Method: PATCH
URL: /api/configuration/chassis0/slots/.*/module/ports/port.*/e1
Body:

    {
      \"objects\": \"new-values\"
    }

Example using curl:

    curl -X PATCH /api/configuration/chassis0/slots/.*/module/ports/port.*/e1
    -d "{
      \"objects\": \"new-values\"
    }"