configuration / chassis0 / slots / [SLOT-ID] / [gns181_uc] / module / ppo
CLI REST-API

## ppo1

The submenu ppo1 (PPO1) contains the following:
Menus:
timer (Timer)
Objects:
length-s (length seconds)
length-ms (length milli-seconds)
output-level (output level)
output-holdover (output holdover (if sync))
mode (mode)
timeout (timeout)
Commands: none

#### Applies to modules

GPS167
GPS167SV
GPS170
GPS180
GNS181_UC
GPS190
GNS181
GNS190
See also:
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/ppo/ppo[ID]/timer
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/ppo/ppo[ID]/length-s
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/ppo/ppo[ID]/length-ms
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/ppo/ppo[ID]/output-level
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/ppo/ppo[ID]/output-holdover
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/ppo/ppo[ID]/mode
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/ppo/ppo[ID]/timeout

#### REST-API Support:

This menu is supported by the REST API:
Method: GET
URL: /api/configuration/chassis0/slots/.*/module/ppo/ppo.*
Example using curl:

    curl /api/configuration/chassis0/slots/.*/module/ppo/ppo.*

Method: PATCH
URL: /api/configuration/chassis0/slots/.*/module/ppo/ppo.*
Body:

    {
      \"objects\": \"new-values\"
    }

Example using curl:

    curl -X PATCH /api/configuration/chassis0/slots/.*/module/ppo/ppo.*
    -d "{
      \"objects\": \"new-values\"
    }"