configuration / chassis0 / slots / [SLOT-ID] / [hps100] / module / ptpv2 / instances / instance[ID] / global / power-ieee-c37-238-2011
CLI REST-API

## network-incaccuracy-nano

network-incaccuracy-nano
This is a read-write object and valid values are unsigned integers.
Datatype-Help:
value must be an unsigned number.

#### Applies to modules

HPS100
See also:
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global/power-ieee-c37-238-2011
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global/power-ieee-c37-238-2011/use-profile-extensions
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global/power-ieee-c37-238-2011/grandmaster-id

#### REST-API Support:

This object is supported by the REST API:
Method: GET
URL: /api/configuration/chassis0/slots/.*/module/ptpv2/instances/instance.*/global/power-ieee-c37-238-2011
Example using curl:

    curl /api/configuration/chassis0/slots/.*/module/ptpv2/instances/instance.*/global/power-ieee-c37-238-2011

Method: PATCH
URL: /api/configuration/chassis0/slots/.*/module/ptpv2/instances/instance.*/global/power-ieee-c37-238-2011
Body:

    {
      "network-incaccuracy-nano": 0
    }

Example using curl:

    curl -X PATCH /api/configuration/chassis0/slots/.*/module/ptpv2/instances/instance.*/global/power-ieee-c37-238-2011 -d
    {
      "network-incaccuracy-nano": 0
    }