configuration / network / ports / lan[ID]
CLI REST-API

## mac-address

MAC Address
This is a read-write object and valid values are MAC-addresses.
Datatype-Help:
the hex-string should looks like this: AA:BB:CC:DD:EE:FF
every letter is a hex-digit.
valid hex-digits are: 0-9 and a-f.
example: 01:23:45:67:89:ab
See also:
/configuration/network/ports/lan[ID]
/configuration/network/ports/lan[ID]/net-link
/configuration/network/ports/lan[ID]/link-led
/configuration/network/ports/lan[ID]/bonding
/configuration/network/ports/lan[ID]/ipv6-mode
/configuration/network/ports/lan[ID]/prp-group
/status/network/ports/lan[ID]/mac-address

#### REST-API Support:

This object is supported by the REST API:
Method: GET
URL: /api/configuration/network/ports/lan.*
Example using curl:

    curl /api/configuration/network/ports/lan.*

Method: PATCH
URL: /api/configuration/network/ports/lan.*
Body:

    {
      "mac-address": "00:00"
    }

Example using curl:

    curl -X PATCH /api/configuration/network/ports/lan.* -d
    {
      "mac-address": "00:00"
    }