configuration / services / network / vif[ID]
CLI REST-API

## snmp

snmp
This is a read-write object and valid values are:

- no [0]
- yes [1]

See also:
/configuration/notification/events/[EVENT-ID]
/configuration/notification/events/[EVENT-ID]/mms
/configuration/notification/events/[EVENT-ID]/email: email
/configuration/notification/events/[EVENT-ID]/disp
/configuration/notification/events/[EVENT-ID]/user

#### REST-API Support:

This object is supported by the REST API:
Method: GET
URL: /api/configuration/services/network/vif.*
Example using curl:

    curl /api/configuration/services/network/vif.*

Method: PATCH
URL: /api/configuration/services/network/vif.*
Body:

    {
      "snmp": true
    }

Example using curl:

    curl -X PATCH /api/configuration/services/network/vif.* -d
    {
      "snmp": true
    }

Valid values when accessing this object via REST API/JSON: false [0], true [1]