configuration / chassis0 / slots / [SLOT-ID] / [gps190] / module / ssm
CLI REST-API

## time-to-restore

Time to Restore
This is a read-write object and valid values are signed integers.
Datatype-Help:
value must be a signed number.

#### Applies to modules

GPS167
GPS167SV
GPS170
GPS180
GNS181_UC
GPS190
GNS181
GNS190
See also:
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/ssm
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/ssm/holdoff-time

#### REST-API Support:

This object is supported by the REST API:
Method: GET
URL: /api/configuration/chassis0/slots/.*/module/ssm
Example using curl:

    curl /api/configuration/chassis0/slots/.*/module/ssm

Method: PATCH
URL: /api/configuration/chassis0/slots/.*/module/ssm
Body:

    {
      "time-to-restore": 0
    }

Example using curl:

    curl -X PATCH /api/configuration/chassis0/slots/.*/module/ssm -d
    {
      "time-to-restore": 0
    }