status / chassis0 / slots / [SLOT-ID] / [hps100] / module / ptpv2 / instances / instance[ID] / datasets / port
CLI REST-API

## announce-receipt-timeout

shall be an integral multiple of log-announce-interval
This is a read-only object and valid values are unsigned integers within a range of 2-10.

#### Applies to modules

HPS100
See also:
/status/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/datasets/port
/status/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/datasets/port/port-state
/status/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/datasets/port/log-min-delay-req-interval
/status/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/datasets/port/log-announce-interval
/status/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/datasets/port/log-sync-interval
/status/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/datasets/port/delay-mechanism
/status/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/datasets/port/log-min-pdelay-req-interval
/status/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/datasets/port/version-number

#### REST-API Support:

This object is supported by the REST API:
Method: GET
URL: /api/status/chassis0/slots/.*/module/ptpv2/instances/instance.*/datasets/port
Example using curl:

    curl /api/status/chassis0/slots/.*/module/ptpv2/instances/instance.*/datasets/port