configuration / chassis0 / slots / [SLOT-ID] / [gps180] / module
CLI REST-API

## tcr

The submenu tcr (TCR) contains the following:
Menus: none
Objects:
utc-offset-sign (UTC Offset Sign)
utc-offset-hours (UTC Offset hours)
utc-offset-minutes (UTC Offset minutes)
irig-code (IRIG Code)
ignore-lock (Ignore Lock)
enable-pulses (Enable Pulses)
irig-tfom-input (IRIG TFOM Input (-1 = disabled))
irig-tfom-output (IRIG TFOM Output (-1 = disabled))
Commands: none

#### Applies to modules

GPS167
GPS167SV
GPS170
GPS180
GNS181_UC
GPS190
GNS181
GNS190
See also:
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/tcr/utc-offset-sign
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/tcr/utc-offset-hours
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/tcr/utc-offset-minutes
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/tcr/irig-code
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/tcr/ignore-lock
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/tcr/enable-pulses
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/tcr/irig-tfom-input
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/tcr/irig-tfom-output

#### REST-API Support:

This menu is supported by the REST API:
Method: GET
URL: /api/configuration/chassis0/slots/.*/module/tcr
Example using curl:

    curl /api/configuration/chassis0/slots/.*/module/tcr

Method: PATCH
URL: /api/configuration/chassis0/slots/.*/module/tcr
Body:

    {
      \"objects\": \"new-values\"
    }

Example using curl:

    curl -X PATCH /api/configuration/chassis0/slots/.*/module/tcr
    -d "{
      \"objects\": \"new-values\"
    }"