configuration / chassis0 / slots / [SLOT-ID] / [gps167sv] / module / gps / serial-ports
CLI REST-API

## com0

The submenu com0 (com0) contains the following:
Menus: none
Objects:
baudrate (Baudrate)
framing (Framing)
mode (Mode)
string-type (String Type)
Commands: none

#### Applies to modules

GPS167
GPS167SV
GPS170
GPS180
GNS181_UC
GPS190
GNS181
GNS190
See also:
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/gps/serial-ports/com[ID]/baudrate
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/gps/serial-ports/com[ID]/framing
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/gps/serial-ports/com[ID]/mode
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/gps/serial-ports/com[ID]/string-type

#### REST-API Support:

This menu is supported by the REST API:
Method: GET
URL: /api/configuration/chassis0/slots/.*/module/gps/serial-ports/com.*
Example using curl:

    curl /api/configuration/chassis0/slots/.*/module/gps/serial-ports/com.*

Method: PATCH
URL: /api/configuration/chassis0/slots/.*/module/gps/serial-ports/com.*
Body:

    {
      \"objects\": \"new-values\"
    }

Example using curl:

    curl -X PATCH /api/configuration/chassis0/slots/.*/module/gps/serial-ports/com.*
    -d "{
      \"objects\": \"new-values\"
    }"