configuration / network / interfaces / vif[ID]
CLI REST-API

## vlan

The submenu vlan (vlan) contains the following:
Menus: none
Objects:
enable-vlan (enable vlan)
vlan-id (vlan-id (0-4094))
priority (priority)
Commands: none
See also:
/configuration/network/interfaces/vif[ID]/vlan/enable-vlan
/configuration/network/interfaces/vif[ID]/vlan/vlan-id
/configuration/network/interfaces/vif[ID]/vlan/priority

#### REST-API Support:

This menu is supported by the REST API:
Method: GET
URL: /api/configuration/network/interfaces/vif.*/vlan
Example using curl:

    curl /api/configuration/network/interfaces/vif.*/vlan

Method: PATCH
URL: /api/configuration/network/interfaces/vif.*/vlan
Body:

    {
      \"objects\": \"new-values\"
    }

Example using curl:

    curl -X PATCH /api/configuration/network/interfaces/vif.*/vlan
    -d "{
      \"objects\": \"new-values\"
    }"