configuration / chassis0 / slots / [SLOT-ID] / [gps170] / module / mrs / xmulti / alt-priority1
CLI REST-API

## refclk0

Refclk0
This is a read-write object and valid values are signed integers.
Datatype-Help:
value must be a signed number.

#### Applies to modules

GPS167
GPS167SV
GPS170
GPS180
PZF180
GNS181_UC
GPS190
GNS181
GNS190
See also:
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/mrs/xmulti/alt-priority1
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/mrs/xmulti/alt-priority1/refclk1
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/mrs/xmulti/alt-priority1/refclk2
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/mrs/xmulti/alt-priority1/refclk3
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/mrs/xmulti/alt-priority1/refclk4
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/mrs/xmulti/alt-priority1/refclk5
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/mrs/xmulti/alt-priority1/refclk6
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/mrs/xmulti/alt-priority1/refclk7
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/mrs/xmulti/alt-priority1/refclk8
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/mrs/xmulti/alt-priority1/refclk9

#### REST-API Support:

This object is supported by the REST API:
Method: GET
URL: /api/configuration/chassis0/slots/.*/module/mrs/xmulti/alt-priority1
Example using curl:

    curl /api/configuration/chassis0/slots/.*/module/mrs/xmulti/alt-priority1

Method: PATCH
URL: /api/configuration/chassis0/slots/.*/module/mrs/xmulti/alt-priority1
Body:

    {
      "refclk0": 0
    }

Example using curl:

    curl -X PATCH /api/configuration/chassis0/slots/.*/module/mrs/xmulti/alt-priority1 -d
    {
      "refclk0": 0
    }