configuration / network / interfaces / vif[ID] / ipv4
CLI REST-API

## dhcp-client-id

dhcp client id
This is a read-write object and valid values are strings with a length of 0-24.
Datatype-Help:
value must be a string.
the length must be between 0 and 24.
See also:
/configuration/network/interfaces/vif[ID]/ipv4
/configuration/network/interfaces/vif[ID]/ipv4/ip-address
/configuration/network/interfaces/vif[ID]/ipv4/netmask
/configuration/network/interfaces/vif[ID]/ipv4/gateway
/configuration/network/interfaces/vif[ID]/ipv4/enable-dhcp

#### REST-API Support:

This object is supported by the REST API:
Method: GET
URL: /api/configuration/network/interfaces/vif.*/ipv4
Example using curl:

    curl /api/configuration/network/interfaces/vif.*/ipv4

Method: PATCH
URL: /api/configuration/network/interfaces/vif.*/ipv4
Body:

    {
      "dhcp-client-id": "Meinberg"
    }

Example using curl:

    curl -X PATCH /api/configuration/network/interfaces/vif.*/ipv4 -d
    {
      "dhcp-client-id": "Meinberg"
    }