configuration / chassis0 / slots / [SLOT-ID] / [gps167] / module / havequick
CLI REST-API

## rx-format

RX format
This is a read-write object and valid values are:

- stanag4246-1 [0]
- stanag4246-2 [1]
- stanag4246-ptti [2]
- stanag4372-saturn-1 [3]
- stanag4372-saturn-2 [4]
- stanag4430-extd [5]

#### Applies to modules

GPS167
GPS167SV
GPS170
GPS180
GNS181_UC
GPS190
GNS181
GNS190
See also:
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/havequick
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/havequick/tx-format
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/havequick/tx-inverted
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/havequick/tx-gen-local-time
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/havequick/rx-min-tfom
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/havequick/rx-inverted
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/havequick/rx-external-pps
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/havequick/rx-offset

#### REST-API Support:

This object is supported by the REST API:
Method: GET
URL: /api/configuration/chassis0/slots/.*/module/havequick
Example using curl:

    curl /api/configuration/chassis0/slots/.*/module/havequick

Method: PATCH
URL: /api/configuration/chassis0/slots/.*/module/havequick
Body:

    {
      "rx-format": "stanag4246-1"
    }

Example using curl:

    curl -X PATCH /api/configuration/chassis0/slots/.*/module/havequick -d
    {
      "rx-format": "stanag4246-1"
    }