configuration / services / network / vif[ID]
CLI REST-API

## daytime

daytime
This is a read-write object and valid values are:

- disabled [0]
- enabled [1]

See also:
/configuration/services/network/vif[ID]
/configuration/services/network/vif[ID]/ftp
/configuration/services/network/vif[ID]/http
/configuration/services/network/vif[ID]/https
/configuration/services/network/vif[ID]/mbgdevman
/configuration/services/network/vif[ID]/mms
/configuration/services/network/vif[ID]/ntp
/configuration/services/network/vif[ID]/ptp
/configuration/services/network/vif[ID]/snmp
/configuration/services/network/vif[ID]/ssh
/configuration/services/network/vif[ID]/telnet
/configuration/services/network/vif[ID]/time
/configuration/services/network/vif[ID]/webshell

#### REST-API Support:

This object is supported by the REST API:
Method: GET
URL: /api/configuration/services/network/vif.*
Example using curl:

    curl /api/configuration/services/network/vif.*

Method: PATCH
URL: /api/configuration/services/network/vif.*
Body:

    {
      "daytime": true
    }

Example using curl:

    curl -X PATCH /api/configuration/services/network/vif.* -d
    {
      "daytime": true
    }

Valid values when accessing this object via REST API/JSON: false [0], true [1]