configuration / chassis0 / slots / [SLOT-ID] / [hps100] / module
CLI REST-API

## software-ntp

Run additional software NTP daemon
This is a read-write object and valid values are:

- disabled [0]
- enabled [1]

#### Applies to modules

HPS100
See also:
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/baudrate
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/framing
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/mode
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/string-type

#### REST-API Support:

This object is supported by the REST API:
Method: GET
URL: /api/configuration/chassis0/slots/.*/module
Example using curl:

    curl /api/configuration/chassis0/slots/.*/module

Method: PATCH
URL: /api/configuration/chassis0/slots/.*/module
Body:

    {
      "software-ntp": true
    }

Example using curl:

    curl -X PATCH /api/configuration/chassis0/slots/.*/module -d
    {
      "software-ntp": true
    }

Valid values when accessing this object via REST API/JSON: false [0], true [1]