configuration / chassis0 / slots / [SLOT-ID] / [hps100] / module / ptpv2 / instances / instance[ID] / global / telecom-itu-t-g-8275-1
CLI REST-API

## use-profile-extensions

use-profile-extensions
This is a read-write object and valid values are:

- no [0]
- yes [1]

#### Applies to modules

HPS100
See also:
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global/power-ieee-c37-238-2011
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global/power-ieee-c37-238-2011/grandmaster-id
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global/power-ieee-c37-238-2011/network-incaccuracy-nano

#### REST-API Support:

This object is supported by the REST API:
Method: GET
URL: /api/configuration/chassis0/slots/.*/module/ptpv2/instances/instance.*/global/telecom-itu-t-g-8275-1
Example using curl:

    curl /api/configuration/chassis0/slots/.*/module/ptpv2/instances/instance.*/global/telecom-itu-t-g-8275-1

Method: PATCH
URL: /api/configuration/chassis0/slots/.*/module/ptpv2/instances/instance.*/global/telecom-itu-t-g-8275-1
Body:

    {
      "use-profile-extensions": true
    }

Example using curl:

    curl -X PATCH /api/configuration/chassis0/slots/.*/module/ptpv2/instances/instance.*/global/telecom-itu-t-g-8275-1 -d
    {
      "use-profile-extensions": true
    }

Valid values when accessing this object via REST API/JSON: false [0], true [1]