status / chassis0 / slots / [SLOT-ID] / [hps100] / module / ptpv2 / instances / instance[ID] / datasets / default
CLI REST-API

## priority-1

priority 1 attribute for the local clock
This is a read-only object and valid values are unsigned integers within a range of 0-255.

#### Applies to modules

HPS100
See also:
/status/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/datasets/default
/status/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/datasets/default/number-ports
/status/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/datasets/default/priority-2
/status/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/datasets/default/clock-identity
/status/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/datasets/default/domain-number

#### REST-API Support:

This object is supported by the REST API:
Method: GET
URL: /api/status/chassis0/slots/.*/module/ptpv2/instances/instance.*/datasets/default
Example using curl:

    curl /api/status/chassis0/slots/.*/module/ptpv2/instances/instance.*/datasets/default