status / chassis0 / slots / [SLOT-ID] / [pzf600] / module / dcf77 / receiver
CLI REST-API

## invalid-time

invalid time because battery had been disconnected, or absolute time can not be decoded safely
This is a read-only object and valid values are:

- no [0]
- yes [1]

#### Applies to modules

PZF511
AM511
PZF600
PZF180
See also:
/status/chassis0/slots/[SLOT-ID]/[am511]/module/dcf77/receiver
/status/chassis0/slots/[SLOT-ID]/[am511]/module/dcf77/receiver/freerunning
/status/chassis0/slots/[SLOT-ID]/[am511]/module/dcf77/receiver/daylight-savings-time
/status/chassis0/slots/[SLOT-ID]/[am511]/module/dcf77/receiver/synchronized-after-reset
/status/chassis0/slots/[SLOT-ID]/[am511]/module/dcf77/receiver/daylight-savings-time-announced
/status/chassis0/slots/[SLOT-ID]/[am511]/module/dcf77/receiver/utc-timescale
/status/chassis0/slots/[SLOT-ID]/[am511]/module/dcf77/receiver/leapsecond-announced
/status/chassis0/slots/[SLOT-ID]/[am511]/module/dcf77/receiver/manual-time

#### REST-API Support:

This object is supported by the REST API:
Method: GET
URL: /api/status/chassis0/slots/.*/module/dcf77/receiver
Example using curl:

    curl /api/status/chassis0/slots/.*/module/dcf77/receiver

Valid values when accessing this object via REST API/JSON: false [0], true [1]