configuration / chassis0 / slots / [SLOT-ID] / [gns181] / module / tcr
CLI REST-API

## utc-offset-hours

UTC Offset hours
This is a read-write object and valid values are signed integers within a range of 0-23.
Datatype-Help:
value must be between 0 and 23.

#### Applies to modules

GPS167
GPS167SV
GPS170
GPS180
GNS181_UC
GPS190
GNS181
GNS190
See also:
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/tcr
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/tcr/utc-offset-sign
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/tcr/utc-offset-minutes
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/tcr/irig-code
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/tcr/ignore-lock
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/tcr/enable-pulses
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/tcr/irig-tfom-input
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/tcr/irig-tfom-output

#### REST-API Support:

This object is supported by the REST API:
Method: GET
URL: /api/configuration/chassis0/slots/.*/module/tcr
Example using curl:

    curl /api/configuration/chassis0/slots/.*/module/tcr

Method: PATCH
URL: /api/configuration/chassis0/slots/.*/module/tcr
Body:

    {
      "utc-offset-hours": 0
    }

Example using curl:

    curl -X PATCH /api/configuration/chassis0/slots/.*/module/tcr -d
    {
      "utc-offset-hours": 0
    }