status / chassis0 / slots / [SLOT-ID] / [gps167sv] / module / satellites / gnss / satellite-list / [ID]
CLI REST-API

## azimuth

azimuth in degrees
This is a read-only object and valid values are signed integers within a range of -32768-32767.

#### Applies to modules

GPS167
GPS167SV
GPS170
GRC170
MGR170
GPS180
GLN170
MGR180
GRC180
GRC181
GNS181_UC
GPS190
GNS181
GNM181
GNS190
See also:
/status/chassis0/slots/[SLOT-ID]/[gln170]/module/satellites/gps/satellite-list/[ID]
/status/chassis0/slots/[SLOT-ID]/[gln170]/module/satellites/gps/satellite-list/[ID]/svno
/status/chassis0/slots/[SLOT-ID]/[gln170]/module/satellites/gps/satellite-list/[ID]/elevation
/status/chassis0/slots/[SLOT-ID]/[gln170]/module/satellites/gps/satellite-list/[ID]/doppler
/status/chassis0/slots/[SLOT-ID]/[gln170]/module/satellites/gps/satellite-list/[ID]/selected

#### REST-API Support:

This object is supported by the REST API:
Method: GET
URL: /api/status/chassis0/slots/.*/module/satellites/gnss/satellite-list/.*
Example using curl:

    curl /api/status/chassis0/slots/.*/module/satellites/gnss/satellite-list/.*