status / network / ports / lan[ID]
CLI REST-API

## port-id

port index of the card
This is a read-only object and valid values are signed integers.
See also:
/status/network/ports/lan[ID]
/status/network/ports/lan[ID]/port-available: port is available
/status/network/ports/lan[ID]/duplex
/status/network/ports/lan[ID]/operstate
/status/network/ports/lan[ID]/speed
/status/network/ports/lan[ID]/mac-address
/status/network/ports/lan[ID]/link
/status/network/ports/lan[ID]/slot-id: identification number of the slot, where the card is
/status/network/ports/lan[ID]/slot-name: name of the slot, where the card is
/status/network/ports/lan[ID]/card-name: name of the card

#### REST-API Support:

This object is supported by the REST API:
Method: GET
URL: /api/status/network/ports/lan.*
Example using curl:

    curl /api/status/network/ports/lan.*