configuration / chassis0 / slots / [SLOT-ID] / [hps100] / module / ptpv2 / instances / instance[ID] / network
CLI REST-API

## dscp-ptp-classification

dscp-ptp-classification
This is a read-write object and valid values are:

- deactivated [-1]
- cs1 [8]
- af11 [10]
- af12 [12]
- af13 [14]
- cs2 [16]
- af21 [18]
- af22 [20]
- af23 [22]
- cs3 [24]
- af31 [26]
- af32 [28]
- af33 [30]
- cs4 [32]
- af41 [34]
- af42 [36]
- af43 [38]
- cs5 [40]
- ef [46]
- cs6 [48]
- cs7 [56]
- custom-00 [0]
- custom-01 [1]
- custom-02 [2]
- custom-03 [3]
- custom-04 [4]
- custom-05 [5]
- custom-06 [6]
- custom-07 [7]
- custom-09 [9]
- custom-11 [11]
- custom-13 [13]
- custom-15 [15]
- custom-17 [17]
- custom-19 [19]
- custom-21 [21]
- custom-23 [23]
- custom-25 [25]
- custom-27 [27]
- custom-29 [29]
- custom-31 [31]
- custom-33 [33]
- custom-35 [35]
- custom-37 [37]
- custom-39 [39]
- custom-41 [41]
- custom-42 [42]
- custom-43 [43]
- custom-44 [44]
- custom-45 [45]
- custom-47 [47]
- custom-49 [49]
- custom-50 [50]
- custom-51 [51]
- custom-52 [52]
- custom-53 [53]
- custom-54 [54]
- custom-55 [55]
- custom-57 [57]
- custom-58 [58]
- custom-59 [59]
- custom-60 [60]
- custom-61 [61]
- custom-62 [62]
- custom-63 [63]

#### Applies to modules

HPS100
See also:
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/network
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/network/net-link-mode
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/network/prp-mac-address-mode
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/network/hostname
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/network/domainname
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/network/nameserver-0
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/network/nameserver-1
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/network/ipv4-address
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/network/ipv4-netmask
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/network/ipv4-gateway
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/network/ipv4-default-gateway
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/network/ipv6-mode
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/network/ipv6-address
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/network/ipv6-gateway
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/network/ipv6-default-gateway
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/network/ipv6-multicast-scope
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/network/multicast-ttl
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/network/dhcp-client
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/network/vlan-enabled
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/network/vlan-id
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/network/vlan-priority

#### REST-API Support:

This object is supported by the REST API:
Method: GET
URL: /api/configuration/chassis0/slots/.*/module/ptpv2/instances/instance.*/network
Example using curl:

    curl /api/configuration/chassis0/slots/.*/module/ptpv2/instances/instance.*/network

Method: PATCH
URL: /api/configuration/chassis0/slots/.*/module/ptpv2/instances/instance.*/network
Body:

    {
      "dscp-ptp-classification": "deactivated"
    }

Example using curl:

    curl -X PATCH /api/configuration/chassis0/slots/.*/module/ptpv2/instances/instance.*/network -d
    {
      "dscp-ptp-classification": "deactivated"
    }