configuration / chassis0 / slots / [SLOT-ID] / [gps190] / module / mrs / xmulti / priority / priority[ID] / feature
CLI REST-API

## auto-bias-master

Auto Bias Master
This is a read-write object and valid values are:

- no [0]
- yes [1]

#### Applies to modules

GPS167
GPS167SV
GPS170
GPS180
PZF180
GNS181_UC
GPS190
GNS181
GNS190
See also:
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/mrs/xmulti/priority/priority[ID]/feature
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/mrs/xmulti/priority/priority[ID]/feature/auto-bias-slave
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/mrs/xmulti/priority/priority[ID]/feature/asymmetry-step-detection
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/mrs/xmulti/priority/priority[ID]/feature/is-trusted-src
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/mrs/xmulti/priority/priority[ID]/feature/use-trusted-src
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/mrs/xmulti/priority/priority[ID]/feature/is-time-of-day-src
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/mrs/xmulti/priority/priority[ID]/feature/is-phase-src
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/mrs/xmulti/priority/priority[ID]/feature/enable-auto-select

#### REST-API Support:

This object is supported by the REST API:
Method: GET
URL: /api/configuration/chassis0/slots/.*/module/mrs/xmulti/priority/priority.*/feature
Example using curl:

    curl /api/configuration/chassis0/slots/.*/module/mrs/xmulti/priority/priority.*/feature

Method: PATCH
URL: /api/configuration/chassis0/slots/.*/module/mrs/xmulti/priority/priority.*/feature
Body:

    {
      "auto-bias-master": true
    }

Example using curl:

    curl -X PATCH /api/configuration/chassis0/slots/.*/module/mrs/xmulti/priority/priority.*/feature -d
    {
      "auto-bias-master": true
    }

Valid values when accessing this object via REST API/JSON: false [0], true [1]