status / chassis0 / slots / [SLOT-ID] / [hps100] / module / ptpv2 / instances / instance[ID] / datasets
CLI REST-API

## time-properties

The submenu time-properties (PTPv2 time properties dataset) contains the following:
Menus:
flags (Flags field)
Objects:
current-utc-offset (offset between TAI and UTC in seconds)
time-source (source of time used by the grandmaster clock)
Commands: none

#### Applies to modules

HPS100
See also:
/status/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/datasets/time-properties/flags
/status/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/datasets/time-properties/current-utc-offset
/status/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/datasets/time-properties/time-source

#### REST-API Support:

This menu is supported by the REST API:
Method: GET
URL: /api/status/chassis0/slots/.*/module/ptpv2/instances/instance.*/datasets/time-properties
Example using curl:

    curl /api/status/chassis0/slots/.*/module/ptpv2/instances/instance.*/datasets/time-properties